|  |  |  |
| --- | --- | --- |
| **Feature Categories** | **Product Features** | **Concept** |
| Performance | -Vertically reciprocating, simplex, positive displacement pump  -Pneumatic  -Consists of 5 parts  -Inflate and pop a water baloon |  |
| Dimensions | Base  Housing  Cover  Piston  Valve |
| Cost | Refer to the TAFE materials pricing chart |
| Standards/Documentations | Pump requirement Specification |
| Product Life | >65 million revolutions |